**PORSCHE CLUB of WA Scrutineering Checksheet**

|  |  |  |
| --- | --- | --- |
| **Date** | **Event** | **Entrant** |
| 16th May 2021 | PCWA SSR4 – Wanneroo Raceway Sprint |  |
| **Vehicle Model** | **Vehicle Year** | **Vehicle Registration** |
|  |  |  |
| **Licenses** | **Number** | **Expiry** | **Type** | **Check** | **Comment** |
| CAMS |  |  |  |  |  |
| Civil |  |  |  |  |  |
| **Item** | **Detail** | **Pass** | **Fail** | **Comment** |
| Lights | Forward facing glass |  |  | Crossed or covered by film (except windscreen) |
|  | Headlights |  |  |  |
|  | Turn Indicators |  |  |  |
|  | Reverse lights & gear |  |  |  |
|  | Brakes |  |  |  |
| Battery | 150 mm Blue Triangle |  |  | Indicating location of the vehicle battery |
|  | Retained / Connection |  |  |  |
| Fluid leaks | Lubricant / Coolant |  |  |  |
| Throttle close mechanism | Return mechanism |  |  | Return mechanism needed on each throttle |
| Tyres | DOT compliant |  |  |  |
|  | Tread depth |  |  |  |
|  | Race (Slick) tyres |  |  | Yes / No Please circle if Race (Slick) tyres in use |
| Steering | Wheel freeplay |  |  |  |
|  | Bearings / Joints |  |  |  |
| Brakes | Fluid level |  |  |  |
|  | Pedal – not low or spongy |  |  |  |
|  | Pads / Rotors |  |  |  |
|  | Dual circuit braking system |  |  | Pre 1 Jan 1974 exempt |
| Tow hook (front and rear) | Fitted / Accessible |  |  | Internal hole diameter at least 40 mm |
| Harness | Condition |  |  | As required by ‘Schedule I’ |
|  | Mount |  |  |  |
|  | Date |  |  | <= 5 yrs from date on harness |
| Seatbelt | Condition |  |  |  |
|  | Mount |  |  |  |
| Extinguisher | Type minimum 900g |  |  | AS1841 – less than 3 years old, refer to ‘Schedule H’ |
|  | Contents gauge |  |  | In ‘Green Zone’, contents of unit loose, shake to test |
|  | Securely mounted |  |  | Bolted metal bracket |
| Helmet | Compliance |  |  | AS1698 SFI24.1 SA2000 E22 BS6658-85 |
|  | Condition |  |  |  |
| Apparel |  |  |  | Cotton clothing – wrist to ankle |
| Loose items | In vehicle |  |  | Water bottles, spare wheel, jack, tools etc. removed |
|  | Accessories / Camera etc. |  |  | Securely mounted |
|  |  |
| Items requiring attention |  |
| Pass scrutineering |  YES NO |
|  | Bronze scrutineer |  |
| Signature |  |
| Pass re-scrutineering |  YES NO |
|  | Scrutineer |  |
| Signature |  |